

In-Door Return Air Pathway (R.A.P.)

PERFECT BALANCE

A step by step instructions for a door

Description automatically generatedA vent with arrows coming out of it

Description automatically generated

A close-up of a logo

Description automatically generated

[**www.tamtech.com**](http://www.tamtech.com) **● (800) 222 - 5932**

|  |  |
| --- | --- |
| **Outside Dimensions Specifications** | |
| **Product Length:** | 27 ¼” |
| **Grille Length:** | 25” |
| **Height:** | 4 ¾” |
| **Depth:** | 1 5/8” |
| **Color:** | White (Paintable) |
| Fits doors 1 3/8” thick only. Rough Opening 24 ½” x 4” | |
| CFM @ 5 Pascals…...136 CFM | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Part # | Qty | Shipping Dimensions | Act Wt (lbs./oz.) | Dim Wt (lbs.) | Individually Boxed |
| TTi-RAP-Di | 1 | 28 x 5 x 2 | 1.7 | 2 | Yes |
| TTi-RAP-D3 | 3 | 28 x 5 x 6.5 | 4.5 | 5 | Yes |
| TTi-RAP-D18 | 18 | 28 x 22 x 10 | 27.2 | 38 | Yes |
| TTi-RAP-D25 | 25 | 28 x 22 x 10 | 27.2 | 38 | No-Bulk |

**In-Door Return Air Pathway (R.A.P.)**

The R.A.P. is the inexpensive alternative to costly jump ducts or dedicated room fresh air returns.

* **Eliminates pressure imbalances**
* **Allows HVAC systems to run more efficiently and reduce energy consumption**
* **Inexpensive, easy to install, no moving parts**
* **Durable, high impact ABS plastic**
* **Made in the USA**
* **Improved bathroom fan performance**